	[image: MTE Schriftzug]




	
	MTE Meter Test Equipment AG
P.O. Box 7550
CH-6302 Zug / Switzerland

Domicile:
Dammstrasse 16
CH-6300 Zug / Switzerland







	[image: ]
	Page 3 / 3

February 8, 2017 




[bookmark: BkmFormTitle]HYDROCAL 1009
Order sheet including accessories 


	Date
	[bookmark: BkmIhreReferenz][bookmark: BkmVorname][bookmark: BkmName]Version
	Author

	[bookmark: BkmDatum]mm dd, yyyy
	
	Mr./Ms.



[bookmark: BkmBetreff] 
Necessary information and standard accessories
	Pos.
	Description
	Quantity

	010
	Power supply

	
	Nominal voltage version
	Supply voltage
	

	
	120 V -20% +15% AC 50/60Hz
	  96 Vmin ... 138 Vmax AC 50/60Hz
	0

	
	230 V -20% +15% AC 50/60Hz
	184 Vmin ... 264 Vmax AC 50/60Hz
	0

	
	120 V -20% +15% DC
	  96 Vmin ... 138 Vmax DC
	0

	
	230 V -20% +15% DC
	184 Vmin ... 264 Vmax DC
	0

	020
	Connection unit thread

	
	G 1½” DIN ISO 228-1
	0

	
	1½” NPT ANSI B 1.20.1
	0

	030
	Communication interface ETHERNET 10/100Mbit/s

	
	Copper wired - RJ45
		[image: ETHERNET Draht]
	0

	
	Fibre optical - SC Duplex
		[image: ETHERNET Licht]
	0

	040
	Configuration Digital Relay Output 1

	
	|X| Normally Open (Standard)
	|_| Normally Closed
	

	050
	Manual for installation and operation

	
	German
	0

	
	English
	0

	060
	Test certificate

	
	German
	0

	
	English
	0

	
	Russian
	0

	070
	Installation on

	
	new Transformer
	0

	
	old Transformer
	0



Optional accessories
	Pos.
	Description
	Quantity

	110
	On-Board Modem (Analog) with connection cable L = 15 m

	
	[image: On-board modem analogue]
	[image: On-board modem analogue connection cable]
	0

	120
	On-Board Modem (GSM) with connection cable and GSM antenna

	
	[image: On-board modem GSM HYDROCAL 1005_1008]
	[image: On-board modem GSM connection cable]
	[image: On-board modem GSM antenna]
	L = 3 m

	
	
	
	
	0

	
	
	
	
	L = 5 m

	
	
	
	
	0

	130
	On-Board Modem (DNP3)

	
	[image: On-board modem DNP 3]
	0

	140
	On-Board Modem (IEC61850) with patch cable, shielding cover and connection card – Note: only possible with communication interface ETHERNET copper wired - RJ45

	
	[image: HYDROCAL 1003_1005_1008_Offhshore IEC 61850 Modem card 50 V02]
	[image: HYDROCAL 1003_1005_1008_Offhshore ETHERNET Connection Cable]
[image: HYDROCAL 1008_1008 Offshore Shelding Plate IEC 61850]
	[image: HYDROCAL 1005_1008_Offshore ETHERNET RJ45 Adaptercard 138 V01]
[image: HYDROCAL 1005_1008_Offshore ETHERNET RJ45_Opto Adaptercard 139 V01]
	RJ45

	
	
	
	
	0

	
	
	
	
	SC Duplex

	
	
	
	
	0

	150
	Measurement input- and opto-coupler output card

	
	[image: IO Board]
	0

	
	Configuration Analog AC Inputs

	
	Current 0/4 … 20 mA (Standard)
	Voltage 0 … 80 V
	

	
	In1
	In2
	In3
	In4
	In5
	In6
	In1
	In2
	In3
	In4
	In5
	In6
	

	
	|X|
	|X|
	|X|
	|X|
	|X|
	|X|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	





Additional information
	End customer

	Name
	

	Address
	

	Street
	

	City
	

	Country
	

	Substation

	Name
	

	Address
	

	Street
	

	City
	

	Country
	

	Transformer

	Manufacturer
	

	Manufacturing Year
	

	Serial Number
	

	Power Rating [MVA]
	

	Voltage Rating [kV]
	



	Remarks
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